1. **To operate system bypassing fresh water tank.**
   1. Connect Fresh Water supply and open valve. (Located exterior roadside of trailer)
   2. In Equipment Room:
      1. Close Tank Fill Valve
      2. Close Tank Bypass Valve
      3. Close Pump Access Valve
      4. Close Antifreeze Valve
      5. Turn off Pump Switch
      6. Close Isolation Valves
2. **To Fill Fresh Water Tank:**
   1. Connect fresh water supply and open valve.
   2. In Equipment Room: Open Tank Fill Valve.
   3. When tank is full close Tank Fill Valve and Fresh Water Valve.
3. **To operate Fresh Water Tank System:**
   1. Open Tank Bypass Valve
   2. Open Pump Access Valve
   3. Close Antifreeze Valve
   4. Close Tank Fill Valve
   5. Open Isolation Valves
   6. Turn on pump switch (Converter breaker must be on)
4. Connect power and check that breakers and switches are in correct position for operation.
5. Ensure all waste tank termination valves are closed.
6. All toilet, urinal, and sink valves are left open as a factory setting.
   1. Toilet valves are located behind toilets.
   2. Urinal valves located behind access panel below urinals.
   3. Sink valves located in cabinet under sink.
7. Recommendation: Add 1 inch of fresh water to waste tank to charge tank to allow paper and solids to dissolve. Single ply quick dissolving toilet tissue is recommended. We recommend not using double ply on high cloth content tissues as they do not dissolve adequately in the waste tank.
8. Recommendation: For odor control, do not use any products containing formaldehyde. **Use** Rid-X to help dissolve solids and add freshening products such as Pine Sol to waste tank.