1. **To fill fresh water tank:** Connect water supply to fresh water connection.
2. **To** **prime pump:** (Located in the Equipment Room)
   1. Connect water to pump prime valve.
   2. Close tank access valve.
   3. Open pump prime valve(s) allowing system to pressurize.
   4. After 30 seconds, close pump prime valve(s).
   5. Reopen tank access valve.
3. **To operate tank system:** (Located in the Equipment Room)
   1. Close antifreeze valve.
   2. Open pump access valve.
   3. Close crossover valves.
   4. Open hot and cold water valves.
   5. Open isolation valves.
   6. Make sure breaker is turned on for pump (located in breaker box).
   7. Run all showers, toilets, and sinks to get all air out of the system.
4. **On-Demand Hot Water Heater**: (Located in the Equipment Room)
   1. Note: The unit is shipped with (2) 65 lb. LP tanks that must be filled prior to use.
   2. Check LP connections and gas supply.
   3. Open gas valves located in Equipment Room.
   4. Turn breaker on for water heater (located in breaker box).

**Note for LP tank change: Do not bypass the LP pressure regulator.** Always connect any LP tank to the main regulator at the front of the trailer. Bypassing this regulator will cause the water heater(s) to fail and void the warranty.